Program for LED interface with Raspberry pi:

from gpiozero import Button, LED

led = LED(25)

button = Button(21)

while True:

button.wait\_for\_press()

led.on()

print("Pressed")

button.wait\_for\_release()

led.off()

print("Released")